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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
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  TEL/WhatsApp: +86 17622605414
Mail: admin@transformercoilwindingmachine.com
    Web:www.transformercoilwindingmachine.com

NAME：Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM)
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Machine Working Diagram
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Machine Technical Parameters:

Fully Automatic Common Mode Hook Winding Machine（KXAT-80HM）
	No.
	Item category
	Value
	Remark

	1
	Device model:
	KXAT-80HM
	

	2
	Compatible magnetic ring (outer diameter):
	31mm-55mm
	

	3
	Adapt to wire diameter:
	1.0mm-2.5mm
	

	4
	Unilateral line length:
	1200mm
	

	5
	Winding speed:
	Depends on wire diameter and number of turns
	

	6
	Apply winding method:
	3-phase common mode (conventional winding method)
	

	7
	power supply:
	220V/50Hz single-phase AC
	

	8
	Gas source:
	0.55Mpa-0.60Mpa
	

	9
	noise:
	60 decibels
	

	10
	equipment power:
	3KW
	

	11
	Equipment energy consumption:
	0.55°/hour
	

	12
	Use ambient temperature:
	-5°C~40°C
	

	13
	Relative humidity:
	(40～90)%RH
	

	14
	Comprehensive pass rate:
	99.5%
	

	15
	Dimensions:
	Length 3050mm (including belt line) * width 1150mm * height 2050mm
	

	16
	Total Weight:
	800KG
	


Machine Winding Product Display

Sample:

phase common mode T60*30*19 wire diameter 2.5mm, 13 turns on one side, 2 layers 

Actual production capacity = 105 pieces/hour
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Machine Configuration List:

	No.
	Name
	Brand
	Unit
	Quantity
	Remark

	1
	Equipment cover sheet metal parts
	Non-standard customization
	SET
	1
	

	2
	Machined parts
	Non-standard customization
	SET
	1
	

	3
	Magnetic ring feeding vibration plate, belt line part
	Non-standard customization
	SET
	1
	

	4
	Guide screw (TBI)
	TBI
	SET
	1
	

	5
	Servo motor (Inovance)
	Inovance
	SET
	6
	

	6
	Pneumatic components (AirTAC)
	AirTAC
	SET
	1
	

	7
	PLC 
	Xinjie
	SET
	1
	

	8
	Touch screen (Weilun)
	Xinjie
	SET
	1
	

	9
	Photoelectric sensor
	OMRON
	SET
	6
	

	10
	Magnetic ring fixture design and processing costs
	Non-standard customization
	SET
	1
	

	11
	Software system
	Non-standard customization
	SET
	1
	

	12
	Equipment one year after-sales service
	
	Item
	1
	


Practical Application :

Training for Customers to Operate Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM)

1.All service engineers with 10 years of experience have received special technical training, including specialized expertise in the Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM), enabling them to effectively handle various breakdown issues specific to this automatic hook winding equipment.

2.We guide users to accurately operate and maintain the Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM)—with focused attention to its hook winding mechanisms, automatic wire tension controls, and digital program settings—while providing free consultation about the production process technology of electronic products, particularly those involving common mode coil manufacturing.

3.To ensure the Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM) operates normally, we conduct dedicated training on its automatic cycle programming, hook alignment calibration, operation protocols, and maintenance requirements through English manuals, model-specific instructional videos, and online guidance, tailored to the unique requirements of this fully automatic common mode hook winding equipment.

Packaging:
Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for Digital CNC Wire Coil Winding Machine, Package it with form and pack paper to guarantee unbroken during the transpot.


2.Wooden case package: For larger scale Digital CNC Wire Coil Winding Machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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Factory:

We, KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD., have been experts in winding machine lines for 28 years, with our advanced product portfolio featuring cutting-edge equipment like the Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM)—a state-of-the-art system engineered for automated hook winding of common mode coils, embodying our technical excellence in precision coil manufacturing solutions.

Our KIOXIA LIGHT RING brand holds authoritative certifications and recognitions, including ISO9001:2015, CE approvals, multiple machine patents (encompassing key innovations in models like the Fully Automatic Common Mode Hook Winding Machine (KXAT-80HM)), and the official designation of "high-tech enterprise" by the government. These credentials fully validate the reliability, automation precision, and technical superiority of our entire product range, reinforcing our commitment to delivering advanced winding solutions for diverse common mode coil production needs.

[image: image7.jpg]


[image: image8.jpg]



⑦Machine switch button: power switch, pause, emergency stop, alarm.





⑥Display screen: software debugging, working interface display.





④The working part of the machine: the feeding clip, the upper feeding clip, the magnetic wrapping and the lower feeding clip.





③Belt line (automatic conveying magnetic ring)





⑤Material bin: coiled products.





② Vibration plate (magnetic ring can be placed)











Wire feeding mechanism: two sets of wires are fed at the same time.





① Placement of the spool (two axes)








KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

